## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### GreArc Parameter - paptlPoint

paptlPoint (PPOINTL) - input Pointer to ArcData array.

Pointer to an array of POINTL structures giving the mid- and end-points of the arc. If the mid-point is coincident with the start or end point, a straight line is drawn from the start point to the end point. If COM_ TRANSFORM is not set, the function expects the array of points to be in screen coordinates.

x X-coordinate of point
y Y-coordinate of point