## ALP Programming Guide and Reference

[prev][next][parent][TOC]

### Operation

    regAL = AL;
    regAH = AH;
    AL  (regAH * imm8 + regAL) AND OFFH;
    AH  0;

Note: imm8 has the value of the instruction's second byte. The second byte under normally assembly of this instruction will be 0A, however, explicit modification of this byte will result in the operation described above and may alter results.