## Input/Output Device Driver Reference

[prev][next][parent][TOC]

### Parity

Determines whether a parity bit exists and, if appropriate, what algorithm determines its value. See ASYNC_SETLINECTRL and ASYNC_GETLINECTRL, which can be found in the OS/2 Physical Device Driver Reference.

Initial Value Even parity
First Level Open No effect
Mode Utility User interface to change the parity characteristics