## MMPM/2 Device Driver Reference

[prev][next][parent][TOC]

### AUDIO_LOAD (44h) - Load DSP Code

Category:
AUDIO_IOCTL_CAT (80h)
Function:
AUDIO_LOAD (44h)
Description:
Load DSP Code

Select an item:

    Description
    Parameter Packet Format
    Data Packet Format
    Remarks

If the LOAD_CODE bit is set in the ulFlags field of the MCI_AUDIO_INIT structure on an AUDIO_INIT request, the application must load the DSP code (specified by the device driver in the abLoadPath field of MCI_AUDIO_INIT) into a buffer and issue an AUDIO_LOAD IOCtl request.