## Display Device Driver Reference for OS/2

[prev][next][parent][TOC]

### Calling The EGA Register Interface

To call EGA register interface functions from an assembly language program, the following actions must be performed:

1.Load the registers with the required parameter values
2.Execute software interrupt 10h.

Values returned by the EGA register interface functions are placed in registers.