## MMPM/2 Device Driver Reference

[prev][next][parent][TOC]

### AUDIO_STATUS (41h) - Pointer to structure

Pointer to structure The data packet parameter is a pointer to the following data structure.

    typedef struct _stat {
      LONG                   lSRate;
      LONG                   lBitsPerSRate;
      LONG                   lBsize;
      SHORT                  sMode;
      SHORT                  sChannels;
      ULONG                  ulFlags;
      ULONG                  ulOperation;
      MCI_AUDIO_CHANGE       rAudioChange;
    } MCI_AUDIO_STATUS;

    typedef   MCI _ AUDIO _ STATUS   FAR   * LPMCI _ AUDIO _ STATUS ;