## ALP Programming Guide and Reference

[prev][next][parent][TOC]

### Notes

This instruction can be used with a LOCK prefix. In order to simplify interface to the processor's bus, the destination operand receives a write cycle without regard to the result of the comparison. DEST is written back if the comparison fails, and SRC is written into the destination otherwise. (The processor never produces a locked read without also producing a locked write.) This instruction is not supported on Intel386 processors.