## Display Device Driver Reference for OS/2

[prev][next][parent][TOC]

### GreEscape DEVESC_SETDRIVERCAPSVALUE - Parameters

hdc (HDC) - input A handle to the device context.

lCode (LONG) - input DEVESC_SETDRIVERCAPSVALUE

lInCount (LONG) - input Number of bytes pointed to by pbInData.

pbInData (PBYTE) - input Pointer to a DRIVERCAPS data structure.

The DRIVERCAPS data structure specifies the driver capability to set.

plOutCount (PLONG) - output Not used.

pbOutData (PBYTE) - output Not used.

rc (LONG) - returns Return Code.

Returns NO_ERROR.