## Using Your DDK

[prev][next][parent][TOC]

### PCMCIA Data/Fax Modem Client Services Driver

Driver Description:

This driver contains the Data/Fax Modem Client Service Driver for OS/2, written to the 2.0 specification level of the PCMCIA Card Service Interface .

Compilers/Assemblers Required:

         IBM Assembly Language Processor      (supplied with the DDK)
         Microsoft C 6.0

Build Instructions:

1.Set the environment variables so the correct tools are picked up during the build.

    e.g., SET PATH=<drive>:\DDK\TOOLS;%PATH%

Where <drive> represents your DDK installed drive and DDK represents the DDK installed directory. On the CD-ROM, the TOOLS directory path is DDK\ TOOLS.

2.Before the FIRST build is attempted, run (only once) the COPYC60.CMD REXX command file in the \DDK\TOOLS directory. This command copies the set of needed files from your copy of the Microsoft C 6.0 compiler to the proper directories under the DDK base directory.

    e.g., COPYC60 <MSCdrive>:\'MSC60' <drive>:\DDK

Where <MSCdrive> represents the Microsoft C 6.0 installed drive and 'MSC60' represents the Microsoft C 6.0 installed directory, <drive> represents your DDK installed drive and DDK represents the DDK installed directory.

3.Change the directory to DDK\BASE\SRC\DEV\PCMCIA\CLDFM.

4.Invoke NMAKE on the resident makefile.

Files Created by Successful Build:

         Directory:  \DDK\BASE\SRC\DEV\PCMCIA\CLDFM

         o  ESTDFM.OS2