## Virtual Device Driver Reference for OS/2

[prev][next][parent][TOC]

### VDHPushInt - Parameters

Vector (ULONG) Number of the interrupt vector to push (0-255).

rc (BOOL) - returns

Success If the function was successful, it returns a nonzero value.

Failure If the function fails, it returns 0 if the client is in protected mode and the stack is invalid or a stack underflow would occur. A stack exception will be simulated to the client. If Vector is invalid, a system halt occurs.