## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### Parameters

ulResetValue (PVOID) - input

Indicates the reset state of the printer. Values are as follows:

Value Description

1 PRTRESET_POWER_ON
Reset printer to power-on condition. For NPAP, this returns the printer to the NPAP-initialized state.

2 PRTRESET_SW_ONLY
Reset BIDI software protocol layer. This reset leaves the rest of the printer and interpreter configuration as is.

3 PRTRESET_POWER_ON_EXIT_SW
Reset printer to power-on condition and exit BIDI software protocol. All temporary resources are lost, according to Power-On-Reset.

4 PRTRESET_EXIT_SW
Reset printer and exit BIDI software protocol. Temporary resources are preserved.

5 PRTRESET_FACTORY_DEFAULTS
Reset printer to factory defaults. All temporary resources are lost, according to Power-On-Reset.

pInData (PVOID) - input

Contains the value from ulResetValue.

pOutData (PVOID) - output

Not used.