## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### SplProtSendCmd Parameter - pfnBaseProtSendCmd

pfnBaseProtSendCmd (PFN) - input Base protocol converter address for ProtSendCmd routine.

This is NULL unless the protocol converter is an extension to the base protocol converter. If not NULL, the extension protocol converter can call the base converter at this address to let the base converter process the command.