## Storage Device Driver Reference

[prev][next][parent][TOC]

### CDROM_CHECKSECTOR

Read Verification Diagnostic Function

This function verifies that the correct record has been read by the device driver. The expected sector value is compared with a doubleword in the input buffer that contains the sector number of the last record read (first doubleword for COOKED buffers and fifth doubleword for RAW buffers). This is a special function that only applies to the IBM Test Disc, tracks 1, 3, and 6.