## Graphics Adapter Device Driver Reference

[prev][next][parent][TOC]

### VIDEOMODEINFO Field - usType

usType (USHORT) Flag indicating mode type.

The following values are valid for this flag:

MODE_FLAG_NOT_MONO 0x0001; Mono-compatible

MODE_FLAG_GRAPHICS 0x0002; Text mode, Graphics

MODE_FLAG_NO_CLR_BRST 0x0004; Disable Color burst

MODE_FLAG_NATIVE 0x0008; Native (advanced function) mode

IGNORE_CLR_BRST 0x0010; Disable color burst; doesn't make sense for this mode

NOT_PLASMA 0x0020; will not work on plasma display

MODE_FLAG_VGA_ENTRY 0x0040; VGA mode, needs clean up