## Virtual Device Driver Reference for OS/2

[prev][next][parent][TOC]

### DOS Settings

The virtual BIOS device driver is responsible for Include/Exclude region support. The DOS setting MEM_INCLUDE_REGIONS gives the user an option to give more space to EMM/XMS. If the user knows that in a particular DOS session an adapter will not be used, then the linear region taken by that adapter can be given to EMM and XMS through MEM_INCLUDE_REGIONS. MEM_ EXCLUDE_REGIONS gives the user an option to restrict EMM and XMS from claiming a particular region. Both these options are provided through DOS settings. These DOS settings are only applicable at DOS session creation time.