## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### GreGetPel Return Value - rc

rc (LONG) - returns Return Code.

This function must return the color index value for the pel, or CLR_NOINDEX if there is no index corresponding to the color. In addition, the handling routine must raise an error when the point is subject to any clipping.

Possible Errors Detected: When an error is detected, the handling routine must call WinSetErrorInfo to post the condition. Error codes for conditions that the handling routine is expected to check include:

PMERR_BITMAP_NOT_SELECTED
PMERR_COORDINATE_OVERFLOW
PMERR_DEV_FUNC_NOT_INSTALLED
PMERR_HDC_BUSY
PMERR_INV_COORD_SPACE
PMERR_INV_COORDINATE
PMERR_INV_HDC
PMERR_INV_LENGTH_OR_COUNT
PMERR_INV_RECT
PMERR_PEL_IS_CLIPPED
PMERR_PEL_NOT_AVAILABLE

Refer to the "Error Explanations" section in the Presentation Manager Programming Reference for further explanation.