## MMPM/2 Device Driver Reference

[prev][next][parent][TOC]

### SHDEntryPoint

Select an item:

    Syntax
    Parameters
    Returns
    Remarks
    Example Code
    Glossary

Each stream handler must provide this entry point, which is used for the PDD to communicate back to the stream handler.

    #include <os2me.h>

    PSHD_COMMON    pCommon;  /*  Pointer to SHD_COMMON. */

    ULONG          rc;       /*  Return codes. */

    rc = SHDEntryPoint(pCommon);