## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### PRTSW Field - flDevice

flDevice (ULONG) Printer device flags.

Values are as follows:

Bit Description

0 PRTSW_DEV_PAGEPRINT_ALERT - 0x00000001
Set if the printer can send alerts when a page has completed printing.

1 PRTSW_DEV_JOBBEGIN_ALERT - 0x00000002
Set if the printer can send alert when a job begins printing.

2 PRTSW_JOBSTACK_ALERT - 0x00000004
Set if the printer can send alert when a job is stacked (completes printing ).

3 PRTSW_TIMED_ALERT - 0x00000008
Set if the printer can send alerts at a given time interval.

4 PRTSW_LU_REQUIRED - 0x00000010
Set if logical unit number is necessary to submit job to correct interpreter. This flag is clear if the datastream should contain the command to switch to correct interpreter.

5 - 31 Reserved; must be clear.