## MMPM/2 Device Driver Reference

[prev][next][parent][TOC]

### MIX_GETCONNECTIONS (60h) - Determine if Line is Enabled

Category:
AUDIO_IOCTL_CAT (80h)
Function:
MIX_GETCONNECTIONS (60h)
Description:
Determine if Line is Enabled

Select an item:

    Description
    Parameter Packet Format
    Data Packet Format
    Returns
    Example Code

This IOCtl enables an application to determine if a particular mixer line is enabled.