## Physical Device Driver Reference

[prev][next][parent][TOC]

### TOUCH_DEVINDEP_SETSELECTMECH (52h) - Type

Type The field in which the selection detection flag (bit) in the status word returned in Function 66h is set or reset:

Bit 0
0 Push harder (default)
1 Lift off
Bit 1
0 First value taken
1 Single-touch algorithm applied
Bit 2
0 First value taken
1 Stable-region algorithm active
Bit 3-F
0 Reserved.