## Printer Device Driver

[prev][next][parent][TOC]

### PolyShortLine

Processes polyshortlines. A pointer to the shortline header is passed. Within the header, start points and stop points are specified. Following the header is an array of Xs (currently 16 bits). The curve starts at x0,y0 and ends at x1,y1. The number of x values is then determined by the absolute value of y1-y1+1. If y1 is greater than y0, y0 is incremented until it equals y1. If y1 is less than y0, y0 is decremented until it equals y1. The current position is not affected by this call.