## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### GreCopyDCLoadData - Parameters

hdc (HDC) - input Handle of target DC.

flCmd (ULONG) - input Flags indicating which fonts to copy.

Valid flags are:

LCID_RANGE_GPI GPI
LCID_RANGE_AVIO AVIO
LCID_RANGE_BOTH GPI and AVIO

hdcSrc (HDC) - input Handle of source DC.

pInstance (PVOID) - input Pointer to instance data.

lFunction (ULONG) - input High-order WORD=flags; low-order WORD= NGreCopyDCLoadData.

fSuccess (BOOL) - returns Return codes.

On completion, the handling routine must return BOOLEAN (fSuccess).

TRUE Successful
FALSE Error