## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### GreCreateBitmap - Parameters

hdc (HDC) - input Device context handle.

pInfoHd (PBITMAPINFOHEADER) - input Pointer to BITMAPINFOHEADER or BITMAPINFOHEADER2 structure for new bit map.

Pointer to either a BITMAPINFOHEADER structure:

cbFix Length in bytes of this structure
cx Bit-map width
cy Bit-map height
cPlanes Number of color planes, 1 if standard format
cBitCount Number of adjacent color bits per pel

Each plane has ((cx*cBitCount+31)/32*4*cy) bytes.

Or pointer to a BITMAPINFOHEADER2 structure:

cbFix Length in bytes of this structure.

cx Bit-map width.

cy Bit-map height.

cPlanes Number of color planes, 1 if standard format.

cBitCount Number of adjacent color bits per pel.

ulCompression Compression scheme used to store the bit map:

BCA_UNCOMP Bit map is uncompressed (the only valid value).

cbImage Length of bit-map storage data in bytes. If the bit map is uncompressed, 0 (default) can be specified for this.

cxResolution Horizontal component of the resolution of the target device; that is, the resolution of the device for which the bit map is intended in the units specified by usUnits. This information enables an application to select from a resource group the bit map that best matches the characteristics of the current output device.

cyResolution Vertical component of the resolution of the target device; that is, the resolution of the device for which the bit map is intended in the units specified by usUnits. This information enables an application to select from a resource group the bit map that best matches the characteristics of the current output device.

cclrUsed The number of color indexes from the color table that are used by the bit map. If it is 0 (default), all the indexes are used. If it is nonzero, only the first cclrUsed entries in the table are accessed by the system; further entries can be omitted.

For standard formats with a cBitCount of 1, 4, or 8 (and cPlanes=1), any indexes beyond cclrUsed are not valid. For example, a bit map with 64 colors can use the 8-bitcount format without having to supply the other 192 entries in the color table. For the 24-bitcount standard format, cclrUsed is the number of colors used by the bit map.

cclrImportant Minimum number of color indexes for satisfactory appearance of the bit map. More colors can be used in the bit map. However, it is not necessary to assign them to the device palette. These additional colors can be mapped to the nearest colors available. Zero (default) means that all entries are mapped. For a 24-bitcount standard format, the cclrImportant colors are also listed in the color table relating to this bit map.

usUnits Units of measure of the horizontal and vertical components of resolution:

BRU_METRIC (Default) Pels per meter.

usReserved Reserved field. If present, it must be 0.

usRecording Recording algorithm, the format in which bit-map data is recorded:

BRA_BOTTOMUP (Default) Scan lines are recorded from bottom to top.

usRendering Halftoning algorithm used to record bit-map data that has been digitally halftoned:

BRH_NOTHALFTONED (Default) Bit-map data not halftoned.

BRH_ERRORDIFFUSION Error diffusion or damped error diffusion algorithm

BRH_PANDA Processing algorithm for noncoded document acquisition

BRH_SUPERCIRCLE Super circle algorithm

cSize1 Size value 1. If BRH_ERRORDIFFUSION is specified in usRendering, cSize1 is the error damping as a percentage in the range 0 - 100. A value of 100% indicates no damping. A value of 0% indicates that any errors are not diffused.

If the BRH_PANDA or BRH_SUPERCIRCLE is specified, cSize1 is the x-dimension of the pattern used in pels.

cSize2 Size value 2. If BRH_ERRORDIFFUSION is specified in usRendering, this parameter is ignored. If the BRH_PANDA or BRH_SUPERCIRCLE is specified , cSize2 is the Y-dimension of the pattern used in pels.

ulColorEncoding Color encoding:

BCE_RGB (Default) Each element in the color array is an RGB2 data type.

ulIdentifier Reserved for applications.

flUsage (ULONG) - input Additional information, used when creating a new bit map. The only defined flag is:

CBM_INIT When set, the pBitmap and paInfo parameters are used to initialize the newly created bit map. If this flag is not set, the bit map initialization is device dependent. It is assumed that sufficient data is supplied to initialize the whole bit map.

Other flags (16 - 31) can be used for special purposes known to be supported by a particular presentation driver.

pBitmap (PBYTE) - input Pointer to bit-map initialization data, starting on a DWORD-aligned address. This data is stored in the order that the coordinates appear on a display screen, that is, the pel in the lower-left corner is the first in the bit map. Pels are scanned to the right and upward from that position. The bits of the first pel are stored beginning with the most significant bits of the first byte. The data for pels in each scan line is packed together tightly. However, all scan lines are padded at the end so that each one begins on a ULONG boundary. That is, 3 bytes of pel data will hold one 24-bit pel, three 8-bit pels, six 4-bit pels, or twenty-four 1-bit pels. If those 3 bytes are the only pel data for that scan line, 1 more byte of zeros would be required to pad the line to a ULONG boundary.

paInfo (PBITMAPINFO) - input Pointer to BITMAPINFO or BITMAPINFO2 structure for initialization data.

Pointer to either a BITMAPINFO structure:

cbFix Length of structure
cx Bit-map width
cy Bit-map height
cPlanes Number of color planes, 1 if standard format
cBitCount Number of adjacent color bits per pel
argbColor[ ] Color table array of RGB structures:
bBlue
bGreen
bRed

Or to a BITMAPINFO2 structure:

cbFix Length in bytes of this structure.

cx Bit-map width.

cy Bit-map height.

cPlanes Number of color planes, 1 if standard format.

cBitCount Number of adjacent color bits per pel.

ulCompression Compression scheme used to store the bit map:

BCA_UNCOMP Bit map is uncompressed (the only valid value).

cbImage Length of bit-map storage data in bytes. If the bit map is uncompressed, 0 (default) can be specified for this.

cxResolution Horizontal component of the resolution of the target device; that is, the resolution of the device for which the bit map is intended in the units specified by usUnits. This information enables an application to select from a resource group the bit map that best matches the characteristics of the current output device.

cyResolution Vertical component of the resolution of the target device; that is, the resolution of the device for which the bit map is intended in the units specified by usUnits. This information enables an application to select from a resource group the bit map that best matches the characteristics of the current output device.

cclrUsed The number of color indexes from the color table that are used by the bit map. If it is 0 (default), all the indexes are used. If it is nonzero, only the first cclrUsed entries in the table are accessed by the system; further entries can be omitted.

For standard formats with a cBitCount of 1, 4, or 8 (and cPlanes=1), any indexes beyond cclrUsed are not valid. For example, a bit map with 64 colors can use the 8-bitcount format without having to supply the other 192 entries in the color table. For the 24-bitcount standard format, cclrUsed is the number of colors used by the bit map.

cclrImportant Minimum number of color indexes for satisfactory appearance of the bit map. More colors can be used in the bit map but it is not necessary to assign them to the device palette. These additional colors can be mapped to the nearest colors available. Zero (the default) means that all entries are important. For a 24-bitcount standard format, the cclrImportant colors are also listed in the color table relating to this bit map.

usUnits Units of measure of the horizontal and vertical components of resolution:

BRU_METRIC (Default) Pels per meter.

usReserved Reserved field. If present, it must be 0.

usRecording Recording algorithm, the format in which bit-map data is recorded:

BRA_BOTTOMUP (Default.) Scan lines are recorded from bottom to top.

usRendering Halftoning algorithm used to record bit-map data that has been digitally halftoned:

BRH_NOTHALFTONED (Default) Bit-map data not halftoned

BRH_ERRORDIFFUSION Error diffusion or damped error diffusion algorithm

BRH_PANDA Processing algorithm for noncoded document acquisition

BRH_SUPERCIRCLE Super circle algorithm

cSize1 Size value 1. If BRH_ERRORDIFFUSION is specified in usRendering, cSize1 is the error damping as a percentage in the range 0 - 100. A value of 100% indicates no damping. A value of 0% indicates that any errors are not diffused.

If the BRH_PANDA or BRH_SUPERCIRCLE is specified, cSize1 is the X-dimension of the pattern used in pels.

cSize2 Size value 2. If BRH_ERRORDIFFUSION is specified in usRendering, this parameter is ignored. If the BRH_PANDA or BRH_SUPERCIRCLE is specified , cSize2 is the Y-dimension of the pattern used in pels.

ulColorEncoding Color encoding:

BCE_RGB (Default) Each element in the color array is an RGB2 data type.

ulIdentifier Reserved for application use.

argbColor[ ] Color table array of RGB2 structures:

bBlue
bGreen
bRed
fcOptions Reserved. Must be 0.

Note: The same bit-map file format is used for bit maps, icons, and pointers. For details, refer to the Presentation Manager Programming Reference.

pInstance (PVOID) - input Pointer to instance data.

lFunction (ULONG) - input High-order WORD=flags; low-order WORD= NGreCreateBitmap.

rc (HBITMAP) - returns Return codes.

On completion, the handling routine must return the handle of the bit map ( hbm), or 0 if an error occurs.

Possible Errors Detected: Error codes posted by the engine for this function include:

PMERR_DEV_FUNC_NOT_INSTALLED
PMERR_HDC_BUSY
PMERR_INSUFFICIENT_MEMORY
PMERR_INV_BITMAP_DIMENSION
PMERR_INV_HDC
PMERR_INV_INFO_TABLE
PMERR_INV_LENGTH_OR_COUNT
PMERR_INV_SCAN_START
PMERR_INV_USAGE_PARM

Refer to the "Error Explanations" section of the Presentation Manager Programming Reference for further explanation.