## MMPM/2 Device Driver Reference

[prev][next][parent][TOC]

### VSD_INSERTSETTINGSPAGE - Syntax

This command enables a VSD to insert device-specific settings pages into the system configuration application.

hvsd (HVSD) Handle to a VSD instance.

ulFunc (ULONG) Set to VSD_INSERTSETTINGSPAGE.

ulFlags (ULONG) No flags used for this command.

pRequest (PMCI_DEVICESETTINGS_PARMS) Pointer to the MCI_DEVICESETTINGS_ PARMS data structure.

hwndRC (HWND) The return code contains the handle to a settings page or zero if no page is inserted.