## ALP Programming Guide and Reference

[prev][next][parent][TOC]

### ALP4201: Offset operator applied to register-indirect expression

An OFFSET operator was applied to a register-indirect expression. In MASM 5.10 emulation mode this does not cause conversion to an immediate expression; instead the register-indirect addressing mode attributes are retained, and the assembler applies the OFFSET operator to the displacement field, forcing it to have the size of the address offset. Applying the OFFSET operator to a register-indirect expression is illegal if the assembler is not operating under MASM 5.10 emulation.