## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### GreIntersectClipRectangle Parameter - prclRect

prclRect (PRECTL) - input Pointer to rectangle (RECTL structure) in world or device coordinates:

xLeft Minimum x-coordinate of rectangle
yBottom Minimum y-coordinate
xRight Maximum x-coordinate of rectangle
yTop Maximum y-coordinate All the boundaries of the rectangle are inclusive (part of the interior) and are not clipped. If COM_TRANSFORM is not set, the function expects the rectangle to be in device coordinates.