## Virtual Device Driver Reference for OS/2

[prev][next][parent][TOC]

### CMOS Memory Access

CMOS Memory Access provides support for passive reads and writes to virtual CMOS memory. The CMOS portion of the CMOS/RTC can be read or written. The virtual CMOS memory is initialized to the contents of the physical CMOS memory (at the time of DOS session initialization) through the physical clock device driver, which is the physical device driver of the virtual CMOS component. Values are written to the virtual CMOS memory in a buffer local to the DOS session. Unlike the physical CMOS memory, however, the contents of the virtual CMOS memory are lost when the DOS session is terminated.