## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### PRQINFO6 Field - fsType

fsType (USHORT) Queue type.

PRQ3_TYPE_RAW Data is always enqueued in the device specific format.
PRQ3_TYPE_BYPASS Allows the spooler to bypass the queue processor and send data directly to the Printer Driver. Setting this bit allows the spooler to print jobs of type PM_Q_RAW while they are still being spooled.
PRQ3_TYPE_APPDEFAULT This bit is set for the application default queue only .