## Display Device Driver Reference for OS/2

[prev][next][parent][TOC]

### Function 105h - Returns

This function is used to get the DBCS display information associated with the given environment buffer, and returns with AX = ERROR_VIO_INVALID_ LENGTH if the Length specified is less than 2 or the buffer was too short to return all of the DBCS display information. Otherwise, Query DBCS Display Info returns with AX = 0.