## MMPM/2 Device Driver Reference

[prev][next][parent][TOC]

### MSG_REPORTINT

This structure contains fields for the SHC_REPORT_INT message (passed with SpiSendMsg).

    typedef struct _MSG_REPORTINT {

      ULONG     ulMsgLen;      /*  Length of structure. */

      PVOID     pBuffer;       /*  Return pointer. */

      ULONG     ulFlag;        /*  Reason for interrupt. */

      ULONG     ulStatus;      /*  Bytes read or written. */

      ULONG     ulStreamTime;  /*  Stream time in milliseconds. */

    } MSG_REPORTINT;

    typedef   MSG _ REPORTINT   FAR   * PMSG _ REPORTINT ;