## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### GreSetBitmapID - Parameters

hdc (HDC) - input Device context handle.

hbm (HBITMAP) - input Bit-map handle.

lLcid (LONG) - input Local identifier to be associated with the bit map.

pInstance (PVOID) - input Pointer to instance data.

lFunction (ULONG) - input High-order WORD=flags; low-order WORD= NGreSetBitmapID.

rc (BOOL) - returns Return codes.

On completion, the handling routine must return BOOLEAN (fSuccess).

TRUE Successful
FALSE Error

Possible Errors Detected: When an error is detected, the graphics engine calls WinSetErrorInfo to post the condition. Reasons for failure of this function include:

PMERR_BITMAP_IS_SELECTED
PMERR_HBITMAP_BUSY
PMERR_HDC_BUSY
PMERR_INV_HBITMAP
PMERR_INV_HDC

Refer to the "Error Explanations" section of the Presentation Manager Programming Reference for further explanation.