## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### BITMAPINFOHEADER2 Field - cxResolution

cxResolution (ULONG) Horizontal component of the resolution of target device.

The resolution of the device the bit map is intended for, in the units specified by usUnits. This information enables applications to select from a resource group the bit map that best matches the characteristics of the current output device.