## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### SplPdRemoteSetPort - Parameters

hab (HAB) - input Anchor block handle.

pszComputerName (PSZ) - input Name of print server being configured.

pszPortName (PSZ) - input Name of printer port to configure on print server .

Following is an example of a port name:

         LPT1

pflCapabilities (PULONG) - input Pointer to a flag field.

Value is as follows:

FL_ADMIN - 0x00000001 On entry, if this flag is set the administrator wants the remote port settings displayed.

rc (ULONG) - returns Return codes.

0 Success

87(ERROR_INVALID_PARAMETER) An invalid parameter was specified; most likely an invalid pszPortName or pflModified was given.