## ALP Programming Guide and Reference

[prev][next][parent][TOC]

### Description

The SLDT instruction stores the Local Descriptor Table Register (LDTR) in the two-byte register or memory location indicated by the effective address operand. This register is a selector that points into the Global Descriptor Table.

The SLDT instruction is used only in operating system software. It is not used in application programs.