## MMPM/2 Device Driver Reference

[prev][next][parent][TOC]

### VCAI_SETCAPTRECT (6Bh) - Pointer to structure

Pointer to structure The data packet parameter is a pointer to the following data structure.

    typedef struct _VCASETCAPTURERECT {
      ULONG       Source_X_Left;
      ULONG       Source_Y_Top;
      ULONG       Source_Y_Height;
      ULONG       Source_X_Width;
      ULONG       Dest_X_Left;
      ULONG       Dest_Y_Top;
      ULONG       Dest_Y_Height;
      ULONG       Dest_X_Width;
    } VCASETCAPTURERECT;

    typedef   VCASETCAPTURERECT   FAR   *   PVCASETCAPTURERECT ;