## Graphics Adapter Device Driver Reference

[prev][next][parent][TOC]

### BITBLTINFO

BitBlt information structure. BitBlt information structure, used for the GHI_CMD_BITBLT and VMI_CMD_BITBLT. functions.

    typedef struct _BITBLTINFO {

      ULONG         ulLength;       /*  Length of the BITBLTINFO data structure, in bytes. */

      ULONG         ulBltFlags;     /*  Flags for rendering of rasterized data. */

      ULONG         cBlits;         /*  Count of Blts to be performed. */

      ULONG         ulROP;          /*  Raster operation. */

      ULONG         ulMonoBackROP;  /*  Background mix if B_APPLY_BACK_ROP is set. */

      ULONG         ulSrcFGColor;   /*  Monochrome source Foreground color. */

      ULONG         ulSrcBGColor;   /*  Monochrome source Background color and transparent color. */

      ULONG         ulPatFGColor;   /*  Monochrome pattern Foreground color. */

      ULONG         ulPatBGColor;   /*  Monochrome pattern Background color. */

      PBYTE         abColors;       /*  Pointer to color translation table. */

      PBMAPINFO     pSrcBmapInfo;   /*  Pointer to source bit map (BMAPINFO) */

      PBMAPINFO     pDstBmapInfo;   /*  Pointer to destination bit map (BMAPINFO). */

      PBMAPINFO     pPatBmapInfo;   /*  Pointer to pattern bit map (BMAPINFO). */

      PPOINTL       aptlSrcOrg;     /*  Pointer to array of source origin POINTLs. */

      PPOINTL       aptlPatOrg;     /*  Pointer to array of pattern origin POINTLs. */

      PBLTRECT      abrDst;         /*  Pointer to array of Blt rects. */

      PRECTL        prclSrcBounds;  /*  Pointer to source bounding rect of source Blts. */

      PRECTL        prclDstBounds;  /*  Pointer to destination bounding rect of destination Blts. */

    } BITBLTINFO;

    typedef   BITBLTINFO   * PBITBLTINFO ;