## Graphics Adapter Device Driver Reference

[prev][next][parent][TOC]

### VIDEOPMI32Request - Remarks

When issuing this VIDEOPMI32Request, AdapterInfo_cp and VideoModeInfo_cp in VIDEO_ADAPTER should be set to sizeof(ADAPTERINFO) and sizeof(VIDEOMODEINFO ). This way, VIDEOPMI can handle callers built from different sizes of ADAPTERINFO VIDEOMODEINFO and included in different versions of OS/2 Warp.

There is a 16-bit entry point, VIDEOPMI16Request, from VIDEOPMI.DLL for 16- bit callers. It functions exactly the same as its 32-bit counterpart VIDEOPMI32Request. Refer to the VIDEO_ADAPTER data structure in Data Types for format and syntax information.