## MMPM/2 Device Driver Reference

[prev][next][parent][TOC]

### VSD_DDCMD - Remarks

A user-level 32-bit buffer pointer is available in the pProcessLin field of the DDCMDREADWRITE. VSDs should use this pointer if they want to operate on the data while they are not in protect mode. The pBuffer field of the DDCMDREADWRITE contains a pointer whose address type was specified by the VSD on DDCMD_REG_STREAM. When the application returns a buffer, it must return the buffer specified by pBuffer and not by pProcessLin