## Physical Device Driver Reference

[prev][next][parent][TOC]

### KBD_GETSESMGRHOTKEY (76h) - Hot Key ID

Hot Key ID The Hot Key ID. Value is set by the caller. Notice that ID value FFFFh is reserved and should not be used.

A maximum of two of the above bit selections can be chosen for a given hot key definition. If more than two bits are selected or if a reserved bit is selected, the result is an INVALID_PARAMETER error code returned to the caller.