## Physical Device Driver Reference

[prev][next][parent][TOC]

### KBD_SETINTERIMFLAG (52h) - Flag

Flag A 1-byte field containing bit flags. A bit set to 1 indicates the state listed below:

Bit 7 Interim console flag on.
Bit 6 Reserved. Must equal 0.
Bit 5 Program requested on-the-spot conversion.
Bit 4 Reserved. Must equal 0.
Bit 3 Reserved. Must equal 0.
Bit 2 Reserved. Must equal 0.
Bit 1 Reserved. Must equal 0.
Bit 0 Reserved. Must equal 0.