## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### GreQueryRealColors Parameter - pArray

pArray (PLONG) - input Pointer to array in which data is returned.

When LCOLOPT_INDEX is set, this is an array of alternating color indexes and values (in the order, index1, value1, index2, value2 and so on). If there is a color table, colors that are not in the table but are available on the device, have a special index of QLCT_NOTLOADED. In RGB mode, the RGB value is returned in the color indexes.

When LCOLOPT_INDEX is not set, this is an array of color values. Each value is the same as those defined for GreCreateLogColorTable.