## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### SplStdGetBits - Parameters

hstd (HSTD) - input The handle to PM_Q_STD data.

lStart (LONG) - input Offset to the byte at which transfer must start. Used when the data is obtained in a series of calls to SplStdGetBits.

cBytes (LONG) - input The number of bytes to transfer.

pAddress (PCH) - input A pointer to the presentation driver's data buffer.

fSuccess (BOOL) - returns Return codes.

This function returns BOOLEAN (fSuccess).

TRUE Success
FALSE Error