## Physical Device Driver Reference

[prev][next][parent][TOC]

### PRT_GETFRAMECTL (62h) - Returns

The error return code for this function is as follows:

00H Completed successfully

This IOCtl is dependent on the attached printer. If the spooler is active, the CPL/LPI setting by the MODE command does not work and returns error.

IBM-J Printer

The printer device driver supports following combinations of CPL and LPI in the DBCS code page if the spooler is inactive:

       [CPL] 132, 158, 176, 198.

       [LPI] 4, 5, 6, 7 (7.5).

The CPL/LPI setting used by the MODE command does not function correctly in the SBCS code page.

U.S. Printer and ESC/P Printer

The printer device driver supports the following combinations of CPL and LPI, if the spooler is inactive:

       [CPL] 80, 132.

       [LPI] 6, 8.

ESC/P printer

The CPL setting is only effective using ANK characters, but it is not effective using KANJI characters. The implementation is the same as DOS/V.