## ALP Programming Guide and Reference

[prev][next][parent][TOC]

### Notes

If the source operand is in memory, it is automatically converted to the extended-real format.

The performance of the division instructions depends on the PC (Precision Control) field of the FPU control word. If PC specifies a precision of 53 bits, the division instructions will run in 33 clocks. If the specified precision is 24 bits, the division instructions will take only 19 clocks.