## Input/Output Device Driver Reference

[prev][next][parent][TOC]

### Installation

The bidirectional parallel port device driver should be installed to the \ OS2\BOOT directory of the OS/2 partition on your disk. The BASEDEV=PAR1284 .SYS statement must exist in the CONFIG.SYS file. The BASEDEV=PRINT0?.SYS statement (where ? can be 1 or 2 as appropriate) must be removed from the CONFIG.SYS file. The OS/2 operating system must be shutdown and restarted for the bidirectional parallel port device driver to become active.