## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### PRTALERT Field - ulType

ulType (ULONG) Type of alert in a given category.

If ulCategory is PRTALERT_CATEGORY_CORE, the type will be one of the following:

Value Description

1 PRTALERT_TYPE_INPUT - 1
Input alert (for example, out of paper)

2 PRTALERT_TYPE_OUTPUT - 2
Output alert (for example, output bin is full)

3 PRTALERT_TYPE_JAM - 3
Paper jam alert

4 PRTALERT_TYPE_OPERATOR - 4
Operator intervention required (for example, print ribbon jam)

5 PRTALERT_TYPE_CONFIG_CHANGE - 5
Configuration changed (for example, cartridge removed)

6 PRTALERT_TYPE_SUPPLIES - 6
Supplies alert (for example, out of toner)

7 PRTALERT_TYPE_JOB_START - 7
Job started printing

8 PRTALERT_TYPE_JOB_STACKED - 8
Job completed and stacked

9 PRTALERT_TYPE_PAGE_PRINTED - 9
Page printed

10 PRTALERT_TYPE_JOB_CANCELLED - 10
Job cancelled inside printer

11 PRTALERT_TYPE_JOB_HELD - 11
Job held inside printer

12 PRTALERT_TYPE_COVER_OPEN - 12
Cover or panel open.

13 PRTALERT_TYPE_POWER_ON - 13
Printer powered on

14 PRTALERT_TYPE_RESET - 14
Printer reset

15 PRTALERT_TYPE_ONLINE - 15
Printer now online

16 PRTALERT_TYPE_OFFLINE - 16
Printer now offline

17 PRTALERT_TYPE_TIMED_ALERT - 17
Timed alert

18 PRTALERT_TYPE_COMMUNICATION_PROBLEM - 18
Communication problem

19 PRTALERT_TYPE_COMM_STATUS_CHANGED - 19
Communication status changed. BIDI_Q_PORT should be issued to get current state.

0xFFFFFFFF PRTALERT_TYPE_OTHER - 0xFFFFFFFF
Other alert type