## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### SplQmGetJobID - Parameters

hspl (HSPL) - input Spool file handle returned by SplQmOpen.

ulLevel (ULONG) - input Level of job information; currently, level 0 is supported.

pBuf (PVOID) - output Buffer to receive job information.

Level 0 will return the QMJOBINFO data structure. See QMJOBINFO in Data Types for details on this data structure.

cbBuf (ULONG) - input Length of pBuf, in bytes.

pcbNeeded (PULONG) - output Receives length, in bytes, of buffer needed to store job information.

rc (ULONG) - returns Return codes.

0 Success
ERROR_INVALID_HANDLE(6) Invalid handle given.
ERROR_INVALID_PARAMETER(87) ulLevel not 0 or invalid parameter given.
ERROR_MORE_DATA(234) Part of the information requested was returned, but there was not enough room for all the data. The *pcbOutData parameter contains the size of buffer needed to retrieve all the query response data.
ERROR_NOT_SUPPORTED(50) This function is not supported by the print server processing the spool job.
NERR_BufTooSmall(2123) No information was returned because the output buffer was too small. *pcbOutData contains the size of buffer needed to retrieve all the query response data.
NERR_JobNotFound(2151) No spooler job found.