## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### Parameters

pInData (PVOID) - input

Should be set to NULL; for future use.

pOutData (PVOID) - output

Contains the protocol-specific response.

This parameter receives all responses and unknown data from the printer while the passthru session is active.

Note: If TYPE_WITHOUT_WRAPPER is specified, any protocol converter wrapper will be removed before passing the data to the application.