## Display Device Driver Reference for OS/2

[prev][next][parent][TOC]

### Function 106h - Returns

This function returns with AX = 0 if it can successfully get all of the requested registers from the Color Lookup Table. Otherwise, this routine returns with AX = ERROR_VIO_INVALID_PARMS if an invalid color register was requested, or AX = ERROR_VIO_INVALID_LENGTH if too many registers were requested.