## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### SplPdSet Parameter - pInData

pInData (PVOID) - input May contain information required by SplPdSet.

If BIDI_SEND_PASSTHRU is set, this parameter contains the command sequence to pass to the printer and will not be altered by the port driver.

If BIDI_SEND_PASSTHRU is not set, this parameter may contain information required by SplPdSet. See BIDI Command Structures and Command Flow for specific information definitions.